Emisiunea de QTC numarul 2587  din data de 19 august 2026
Apel general pentru emisiunea de QTC, Apel general pentru emisiunea de QTC de  YO3DIU care opereaza pentru YO3KAA
Apel general pentru emisiunea de QTC, Apel general pentru emisiunea de QTC de YO3DIU care opereaza pentru YO3KAA
Astazi vreau sa va prezint QTC-ul numarul 2517 din data de 16 aprilie 2025
Buna ziua, va salut pe toti cei care aveti rabdare sa ma ascultati, eu sper ca informatiile date de mine in acest QTC sa va fie de folos, sau macar sa fie interesante si sa le ascultati ca sa reveniti la aceasta ora si in aceasta frecventa si miercurea viitoare.

Din partea FRR

Rezultatele la concursul Cupa Aviatiei 2026
Citeste din pdf


Comunicat al Comisiei Centrale Tehnice a FRR:

Stimați colegi

Avem placerea să vă anunțăm că anul acesta, Campionatul Național de Creație Tehnică ediția 2026 se va
desfășura sâmbătă 12 septembrie la Izvoru Mureșului, jud. Harghita, în cadrul Complexului Sportiv
Naţional începând cu ora 08:00. Regulamentul competiției poate fi consultat pe saitul hamradio.ro
secțiunea &quot;REGULAMENTE&quot;, tot pe sait fiind disponibile la secțiunea “DOCUMENTE” și Fișele de înscriere
în format editabil. Pentru orice alte detalii rog contactați pe Sorin, YO7CKQ, la telefon 0729 890 806 sau
e-mail yo7ckq@gmail.com
Suplimentar premiilor prevăzute în regulament, competiția beneficiază anul acesta de premii
sponsorizate astfel:
- Locurile I de la categoriile de participare A, B și C vor beneficia de câte un premiu constând într-un
echipament și o mapă promoțională oferite de Dl. Andrei AVIRVAREI, YO6TJJ de la firma roWaves
https://rowaves.com/ro/
- Tot Dl. Andrei AVIRVAREI oferă un pachet surpriză atribuit prin tragere la sorți unuia din participanții la
CNCT ediția 2026
- Firma sigmanortec.ro oferă un voucer de cumpărături în valoare de 400 lei pentru cea mai originlă
lucrare și alte trei în valoare de 350 prin tragere la sorți participanților la CNCT 2026
- Tot prin tragere la sorți se oferă participanților la CNCT 2026:
- o sarcină artificială de 50 ohmi/100 watts sponsorizată de Nelu YO9DL
- o sursă de alimentare profesională de 12 volți/60 amperi sponsorizată de Cristi YO3LR
- Un frecvențmetru digital pentru 100 KHz – 1.2 GHz sponsorizat de Sorin YO7CKQ
Vă reamintim că în aceiași locație se desfășoară Cupa României QRP și tradiționalul Simpo YO ediția
2026. Pentru detalii legate de aceste evenimente vă rugăm să consultați situl FRR, hamradio.ro
Vă mulțumim pentru atenție!

Președinte Comisia Centrală Tehnică, Sorin NIMARĂ, YO7CKQ




YO DX HF Contest
1200Z, Aug 22 to 1200Z, Aug 23
 	Geographic Focus:	Worldwide
 	Participation:	Worldwide
 	Mode:	CW, SSB
 	Bands:	80, 40, 20, 15, 10m
 	Classes:	Single Op All Band Mixed(High/Low)
Single Op All Band CW
Single Op All Band SSB
Single Op Single Band Mixed
Multi-Op Single Transmitter
Youngster/Novice (<18y or licensed for 3 years or less)
SWL
 	Max power:	High: >100W
Low: 100W or less
 	Exchange:	YO: RS(T) + county
non-YO: RS(T) + Serial No.
 	Work stations:	Once per band per mode
 	QSO Points:	YO: 8 points per QSO with non-EU station
YO: 4 points per QSO with non-YO EU station
Non-YO: 8 points per QSO with YO station
Non-YO: 4 points per QSO with non-YO station on different continent
Non-YO: 2 points per QSO with non-YO station in different country, same continent
Non-YO: 1 point per QSO with non-YO station in same country
 	Multipliers:	All: Each DXCC country (not YO) once per band
Non-YO: Each YO county once per band
 	Score Calculation:	Total score = total QSO points x total mults
 	Submit logs by:	1200Z August 30, 2026
 	E-mail logs to:	(none)
 	Upload log at:	https://yodx.ro/upload.php
 	Mail logs to:	(none)
 	Find rules at:	http://www.yodx.ro




Concursuri Romanesti






Concursuri Internationale

Turkiye HF Contest
0600Z, Aug 22 to 0600Z, Aug 23
 	Geographic Focus:	Worldwide
 	Participation:	Worldwide
 	Mode:	CW, SSB
 	Bands:	160, 80, 40, 20, 15, 10m
 	Classes:	Single Op All Band (CW/SSB/Mixed)(QRP/Low/High)
Single Op Single Band (CW/SSB/Mixed)
Multi-Single (Low/High)
 	Max power:	HP: >100 watts
LP: 100 watts
QRP: 5 watts
 	Exchange:	TA: RS + 2-digit province code
non-TA: RS + serial no.
 	Work stations:	Once per band per mode
 	QSO Points:	(see rules)
 	Multipliers:	Each DXCC country once per band
Each province code once per band
 	Score Calculation:	Total score = total QSO points x total mults
 	Submit logs by:	2359Z August 30, 2026
 	E-mail logs to:	(none)
 	Upload log at:	https://tahfcontest.com/
 	Mail logs to:	(none)
 	Find rules at:	https://tahfcontest.com/

ARSI VU DX Contest: 1200Z, Aug 22 to 1200Z, Aug 23
 	Status:	Active, but no recent results
 	Geographic Focus:	India
 	Participation:	Worldwide
 	Mode:	CW, SSB
 	Bands:	40, 20, 15, 10m
 	Classes:	Single Op All Band (CW/SSB/Mixed) (Low/High)
Single Op Single Band (CW/SSB/Mixed) (Low/High)
 	Max power:	HP: >100 watts
LP: 100 watts
 	Exchange:	VU: RS(T) + 2-letter state/UT code
Non-VU: RS(T) + Serial No.
 	Work stations:	Once per band per mode
 	QSO Points:	VU: 1 point per QSO with VU station
VU: 3 points per QSO with DX station
Non-VU: 3 points per QSO with VU station
 	Multipliers:	VU: Each DXCC country once per band per mode
Non-VU: Each VU state/UT once per band per mode
 	Score Calculation:	Total score = total QSO points x total mults
 	Submit logs by:	2359Z August 30, 2026
 	E-mail logs to:	logs[at]arsi[dot]info
 	Mail logs to:	(none)
 	Find rules at:	https://arsi.info/dxcontest/


 	 	 
Hawaii QSO Party: 1600Z, Aug 22 to 0400Z, Aug 24
 	Geographic Focus:	United States/Canada state/province QSO party
 	Participation:	Worldwide
 	Mode:	CW, Phone, Digital
 	Bands:	160, 80, 40, 20, 15, 10m
 	Classes:	Single Op (QRP/Low/High)
Multi-Single (Low/High)
Multi-Multi (Low/High)
 	Max power:	HP: 1500 watts
LP: 100 watts
QRP: 5 watts
 	Exchange:	HI: RS(T) + HI district
non-HI W/VE: RS(T) + (state/province)
DX: RS(T)
 	Work stations:	Once per band per mode
 	QSO Points:	2 points per SSB QSO
3 points per CW/digital QSO
 	Multipliers:	HI: Each HI district once
HI: Each state/province/territory/country once
non-HI: Each HI district once per band
 	Score Calculation:	Total score = total QSO points x total mults
 	Submit logs by:	September 7, 2026
 	E-mail logs to:	ad6e[at]arrl[dot]net
 	Upload log at:	https://hqp.contesting.com/hqpsubmitlog.php
 	Mail logs to:	(none)
 	Find rules at:	http://www.hawaiiqsoparty.org/

CVA DX Contest, SSB: 1800Z, Aug 22 to 2100Z, Aug 23
 	Geographic Focus:	Worldwide
 	Participation:	Worldwide
 	Mode:	SSB
 	Bands:	160, 80, 40, 20, 15, 10m
 	Classes:	Single Op All Band (QRP/Low/High)
Single Op Dual Band (80+10m) Low
Single Op Single Band (Low/High)
Single Op All Band Military (Low/High)
Single Op YL (Low/High)
Multi-Single
Multi-Single Military Fixed
Multi-Single Military Portable
Multi-Two
CVA DX Adventure (see rules)
Overlays: (Rookie/Teen/YL)
 	Max power:	HP: >100 watts
LP: 100 watts
QRP: 5 watts
 	Exchange:	Brazil: RST + state
Non-Brazil: RST + continent
Military: RST + "MIL"
 	Work stations:	Once per band
 	QSO Points:	2 points per QSO with station in same country
3 points per QSO with station in different country/same continent
4 points per QSO with station in different continent
 	Multipliers:	Each Brazilian state once per band
Each country once only
 	Score Calculation:	Total score = total QSO points x total mults
 	Submit logs by:	2359Z August 30, 2026
 	E-mail logs to:	(none)
 	Upload log at:	https://cvadx.org/envio-de-logs-ssb/
 	Mail logs to:	(none)
 	Find rules at:	https://cvadx.org/

SARL HF CW Contest
1400Z-1700Z, Aug 23
 	Geographic Focus:	Southern Africa
 	Participation:	Southern Africa
 	Mode:	CW
 	Bands:	80, 40, 20m
 	Classes:	Single Op Single Radio All Band
Single Op Single Radio Single Band
Multi-Op All Band
Multi-Op Single Band
Overlays (All Classes): YL and Youth
 	Exchange:	RST + Serial No.
 	Score Calculation:	(see rules)
 	Submit logs by:	2159Z August 28, 2026
 	E-mail logs to:	contest[at]sarl[dot]org[dot]za
 	Mail logs to:	(none)
 	Find rules at:	https://mysarl.org.za/contest-resources/


 	 	

	
Rubrica DX

Special event station EN35UKR is active until the 30th of August to mark
the 35th anniversary of Ukraine's independence. QSL via Logbook of the World or direct via UT2UCN.
Curtis, MW0USK and Kevin, MW9KJC are operating as GB64MOD until the 31st of August. The special event station is active to “celebrate the spirit of the Mod movement through amateur radio". Find out more at gb64mod.co.uk

9A10SOTA is the special callsign celebrating ten years of SOTA Croatia. Look out for activity until the 30th of September. QSL via Logbook of the World.

Sands, VK4WXW has returned to Willis Island (OC-007) and will be stationed at the Australian Bureau of Meteorology’s weather monitoring facility until late October or early November. He expects to be increasingly active in the coming weeks and operates SSB and FT8 on the 40, 20, 15 and 10m bands with a vertical antenna. QSL via M0OXO’s OQRS.


Citeste si din buletin…………….DXWorld.net buletin nr 675








Diverse

Thornbury and South Gloucestershire Amateur Radio Club has its annual field weekend on Saturday the 22nd and Sunday the 23rd of August in a field off Hook Street, Berkeley [BARC-LEE] GL13 9TH. All are welcome to visit or catch us on the air, club call sign GX4ABC. For further details, contact the Secretary via email at secretary@tsgarc.uk

Members of the Scarborough Amateur Radio Society will be operating as GB400SCA on the HF Bands between 10am and 4pm on Sunday the 23rd of August from the grounds of Scarborough Castle. The callsign celebrates 'Scarborough 400', marking 400 years since Scarborough became the UK’s original seaside resort when health-giving spa waters were discovered in the cliffs above the beach. This led to the start of seaside tourism in 1626 and the idea of seaside holidays subsequently spread throughout the UK.

Condensatorul Variabil: Sculptura Mecanică ce a Acordat Lumea
​Salutare, dragi prieteni și pasionați ai construcțiilor radio! Ne întâlnim din nou în această seară de miercuri, iar astăzi vă propun să ne oprim privirea asupra unei piese fascinante de pe bancul de lucru. O componentă care îmbină mecanică de precizie și fizică electromagnetică într-un mod spectaculos: condensatorul variabil.
​Pentru cei care au prins epoca de aur a receptoarelor analogice, nimic nu se compară cu senzația tactilă a butonului de acord. Învârteai de acel buton mare, un sistem de scripeți și ațe mișca acul pe scală, iar în interiorul aparatului, un ansamblu de plăci metalice pătrundea lin printre altele, aducând la viață semnale din toate colțurile lumii. Dar cum a apărut această piesă și cum au reușit inginerii să transforme rotația unei axe într-o selectare perfectă a frecvenței?
​Nașterea unei idei: De la sticla de Leyda la aerul dintre plăci
​Până la sfârșitul secolului al XIX-lea, condensatoarele electrice erau piese fixe, fabricate din foi de aluminiu intercalate cu sticlă sau hârtie cerată. Nu puteai regla nimic. Însă odată cu primele experimente de radiotelegrafie ale lui Guglielmo Marconi și Nikola Tesla, s-a născut nevoia arzătoare de a schimba frecvența de rezonanță a circuitelor fără a reconstrui bobinele.
​Inventatorul de origine maghiară Dezso Korda a fost primul care a brevetat, în anul 1893, condensatorul variabil cu dielectric din aer. Ideea lui a fost de o simplitate genială: un set de plăci fixe, numit stator, și un set de plăci mobile, numit rotor, montat pe un ax rotativ. Prin simpla rotire a axului, suprafața de suprapunere dintre plăci se modifica, iar capacitatea electrică se schimba treptat de la câțiva picofarazi la câteva sute de picofarazi.
​Câțiva ani mai târziu, fizicianul englez William Du Bois Duddell a perfecționat această piesă pentru emițătoarele radio, introducând izolații din ceramică și rulmenți de precizie pentru ca valoarea masei electrice să nu fluctueze la cea mai mică vibrație.
​Forma plăcilor și arta acordului liniar
​La prima vedere, toate condensatoarele variabile par la fel. Dacă privim însă cu atenție picioarele din aluminiu ale rotorului, descoperim o adevărată lecție de inginerie.
​Primele condensatoare aveau plăci perfect semicirculare. Aceasta înseamna că variația capacității era direct proporțională cu unghiul de rotire. Dar în fizică, frecvența unui circuit acordat depinde de rădăcina pătrată a capacității! Din acest motiv, la începutul scalei posturile radio erau îngrămădite unele în altele, iar la capătul scalei erau extrem de distanțate.
​Pentru a rezolva această problemă, proiectanții au creat plăci cu profiluri matematice speciale. Așa au apărut condensatoarele cu frecvență liniară, ale căror plăci rotative au o formă asimetrică, aducând o modificare uniformă a frecvenței la fiecare grad rotit. Pentru un constructor de receptoare, această formă a fost un miracol: scala radio nu mai era aglomerată, ci devenea perfect lizibilă de la un capăt la altul.
​De la emițătoarele navale la radiourile cu tranzistoare
​În funcție de utilizare, condensatorul variabil a îmbrăcat forme impresionante. În etajele finale ale emițătoarelor cu lămpi și în tunerele de antenă de mare putere, plăcile aveau grosimi de câțiva milimetri, iar spațiul dintre ele era generos, de mai bine de un centimetru, pentru a preveni străpungerea și arcul electric la tensiuni de mii de volți. Pentru stabilitate absolută, corpul condensatorului era turnat din duraluminiu sau realizat pe plăci rigide din micanit și ceramică.
​În anii '60, odată cu apariția radiourilor portabile cu tranzistoare, gigantul condensator din aer nu mai avea loc în carcasă. Proiectanții au creat varianta ultra-compactă, în care aerul a fost înlocuit cu foițe microscopice din milar sau polietilenă. Deși erau sensibile la uzură mecanică, aceste piese de doar un centimetru cub au permis miniaturizarea radiourilor care au însoțit generații întregi la plajă sau în drumeții.
​Dragi prieteni, astăzi, în era sintezelor digitale de frecvență și a diodelor varicap, condensatorul variabil cu aer pare o piesă dintr-un muzeu al tehnologiei. Însă pentru un radioamator constructor, o axă din alamă care se rotește fără joc între plăci din aluminiu strălucitor rămâne simbolul pur al acordului radio – o combinație de mecanică fină și fizică curată care a pus bazele comunicării moderne.
​Vă mulțumesc pentru atenție și, ca de obicei... să auzim numai de bine! 73!
